(\*\*\*\*\*\*)

Detector loop conductors shall be No. 14 AWG stranded copper conductors, class B, with Type XLP/USE insulation or shall be No. 14 stranded copper conductors conforming to IMSA 51-3 or IMSA 51-5 requirements.